**7.0 REFERENCES CITED**

Andersen, P., and Stewart, M., 2016, Peer Review of the Northern District Model Version 5 and Predictive Simulations October 10, 2016--Final Report. In files of SJRWMD and SWFWMD, Palatka and Brooksville, FL.

Anderson, M., and Woessner, W., 1992, Applied groundwater modeling--Simulation of Flow and Advective Transport: Academic Press, Inc., San Diego, CA.

ASTM, 2008, D5609, Standard guide for defining boundary conditions in groundwater flow modeling: Copyrighted by ASTM International, 100 Barr Harbor Drive, PO Box C700, West Conshohocken, PA 19428-2959: 4p.

ASTM, 2010, D6170, Standard guide for selecting a groundwater modeling code: Copyrighted by ASTM International, 100 Barr Harbor Drive, PO Box C700, West Conshohocken, PA 19428-2959: 19 p.

ASTM, 2018, D5981, Standard guide for calibrating a groundwater flow model application: Copyrighted by ASTM International, 100 Barr Harbor Drive, PO Box C700, West Conshohocken, PA 19428-2959: 5 p.

Doherty, J., 2010, PEST, Model-independent parameter estimation—User manual (5th ed., with minor revisions): Brisbane, Australia, Watermark Numerical Computing.

Doherty, J.E., and Hunt, R.J., 2010, Approaches to highly parameterized inversion—A guide to using PEST for groundwater-model calibration: U.S. Geological Survey Scientific Investigations Report 2010–5169, 59 p.

GeoHydros, 2014, North Florida numerical groundwater flow model—Limitations and Implication for groundwater resource management: In files of SRWMD, Live Oak, FL.

Geurink, J.S., and Basso, R., 2013, “Development, calibration, and evaluation of the Integrated Northern Tampa Bay Hydrologic Model.” Prepared for Tampa Bay Water and the Southwest Florida Water Management District, Clearwater, FL.

Hill, M., 1994, Five computer programs for testing weighted residuals and calculating linear confidence and predictive intervals on results from the ground-water parameter-estimation computer program MODFLOWP, U.S. Geological Survey Open-File Report 93-481.

-----------, 1998, Methods and guidelines for effective model calibration, U.S. Geological Survey Open-File Report 98-4005.

Knowles, L., Jr., O’Reilly, A.M., and Adamski, J.C., 2002, Hydrogeology and simulated effects of ground-water with­drawals from the Floridan aquifer system in Lake County and in the Ocala National Forest and vicinity, north-central Florida: U.S. Geological Survey Water-Resources Investiga­tions Report 02–4207.

Kuniansky, E. L., 2016. Simulating Groundwater Flow in Karst Aquifers with Distributed Parameter Models— Comparison of Porous-Equivalent Media and Hybrid Flow Approaches. Scientific Investigations Report 2016–5116. Reston, Va.: U.S. Geological Survey.

Miller, J.A., 1986, Hydrologic framework of the Floridan aquifer system in Florida and in parts of Georgia, Alabama, and South Carolina: U.S. Geological Survey Professional Paper 1403-B, 91 p.

Poeter, E., and Hill, M., 1997, Inverse models: A necessary next step in ground-water flow modeling: Ground Water, V. 35, no. 2.

Reilly, T.E., and Harbaugh, A.W., 2004, Guidelines for evaluating ground-water flow models: U.S. Geological Survey Scientific Investigations Report 2004-5038, 30 p.

Sepúlveda, Nicasio, Tiedeman, C.R., O’Reilly, A.M., Davis, J.B., and Burger, Patrick, 2012, Groundwater flow and water budget in the surficial and Floridan aquifer systems in east-central Florida: U.S. Geological Survey Scientific Investigations Report 2012–5161.

Smith, M., Laurine, D., Koren, V., Reed, S., and Zhang, Z., 2003, Hydrologic model calibration strategy accounting for model structure, In: Calibration of watershed Models, Water Science and Application 6, American Geophysical Union, Washington, D.C.